IFC building model
Schema: "IFC4"
Description: "IFC Export"
File name: "NOR-413710050.ifc"
Time stamp: "2026-03-09T09:45:08"
Author: "Unknown"
Organization: "SWS SoftWare-Systeme GmbH"
Preprocessor: "SWS IFC Engine 2.2"
Originating system: "WinDelta PMS 2025"
Authorization: "Unknown Authorizer"
Application: "WinDelta PMS 2025" version "9.50f" identifier "www.sws-online.de" by Organization (no name given)

People and organizations
  Person (no name given) of Organization (no name given)
  Owner history of Person (no name given) of Organization (no name given) | application "WinDelta PMS 2025" version "9.50f" identifier "www.sws-online.de" by Organization (no name given) | change ADDED | created 1773049509 (2026-03-09T09:45:09Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE

Spatial structure
IFCPROJECT "Data"
  IFCSITE "Site" | latitude 51° 42′ 6.487199″ | longitude 8° 46′ 0.8148″ | description "Description of Site"
    IFCBUILDING "Building" | description "Description of Building"
      IFCBUILDINGSTOREY "Building Storey" | elevation 0. | description "Description of Building Storey"
        IFCSPACE "Space" | description "Description of Space"
          contains 1 element
            1 x IFCELECTRICAPPLIANCE | names: "NOR-413710050" | descriptions: "EISWÜRFELBEREITER" | property sets: bSD_PSet_FoodServiceEquipmentIdentityData, bSD_PSet_FoodServiceEquipmentGeneral, bSD_PSet_FoodServiceEquipmentElectrical, bSD_PSet_FoodServiceEquipmentPlumbing, bSD_PSet_FoodServiceEquipmentPlumbing (2)

Property sets
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Concealed = FALSE (IFCBOOLEAN)
    HandicapAccessible = TRUE (IFCBOOLEAN)
    MechanicalVentilationRate = 0 (IFCINTEGER)
    NaturalVentilation = TRUE (IFCBOOLEAN)
    NaturalVentilationRate = 0 (IFCINTEGER)
    OccupancyNumber = 0 (IFCINTEGER)
    OccupancyType = "" (IFCTEXT)
    PubliclyAccessible = TRUE (IFCBOOLEAN)
    Reference = "" (IFCTEXT)
  Pset_Draughting | properties | on 1 object (1 IFCSPACE)
    Color: Red = 0 (IFCINTEGER); Green = 0 (IFCINTEGER); Blue = 0 (IFCINTEGER)
    Layer = "Rooms" (IFCLABEL)
  bSD_PSet_FoodServiceEquipmentIdentityData | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    Description = "EISWÜRFELBEREITER" (IFCTEXT)
    Item Number = "NOR-413710050" (IFCTEXT)
    Manufacturer = "NordCap" (IFCTEXT)
    Model = "SCH-50-L-XSAFE" (IFCTEXT)
    Specification by Manufacturer = "EISWÜRFELBEREITER" (IFCTEXT)
    Weight = 38. (IFCMASSMEASURE)
  bSD_PSet_FoodServiceEquipmentGeneral | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    Depth Actual = 570. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Actual = 880. (IFCLENGTHMEASURE) [MILLI METRE]
    Length Actual = 467. (IFCLENGTHMEASURE) [MILLI METRE]
  bSD_PSet_FoodServiceEquipmentElectrical | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    Cycle = "50Hz" (IFCTEXT)
    Electric power = 0.64 (IFCREAL)
    Electrical Connection Height = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Electrical Connection X = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Electrical Connection Y = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Electrical Remarks = "50Hz" (IFCTEXT)
    Volts = "230V" (IFCTEXT)
  bSD_PSet_FoodServiceEquipmentPlumbing | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    Cold Water Connection Height = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Cold Water Connection X = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Cold Water Connection Y = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Cold Water Size = "3/4"" (IFCTEXT)
  bSD_PSet_FoodServiceEquipmentPlumbing (2) | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    Direct Waste Connection Height (2) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Direct Waste Connection X (2) = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Direct Waste Connection Y (2) = 0. (IFCLENGTHMEASURE) [MILLI METRE]